FVUI V0.11.12（202503192023）Version release log

# Introduction

* **Firmware version:** FVUI\_7628\_V0.12.12\_202503192023\_RC.bin
* **Version upgrade：**Upgrade from V0.11.6（202411022003）to V0.11.12（202503192023）
* **Applicable models:** P10/P10P/P10G/P10LTE/P11/P11P/P11G/P11LTE
* **Release date:** 2025.04.10

# New Features

1. Supports TLS1.3.
2. Add a secondary dial tone.

# Function optimization

1. Support from and P-Asserted-Identity for the caller name display for calls with tel numbers.
2. The call log was expanded to 150 entries each.
3. Add velans xml requirements:

The ringtone should continue after the screen is off;

There should be a sound prompt when an XML message is received in the call;

Exit the soft button to exit directly to the home screen.

1. Add the ringtone playback duration control parameter RingTime.
2. Add feature control to limit whether different server are restricted by the registered suffix.

# Problem fixing

1. Fixed the problem that normal incoming calls could not be transferred after the multicast was transferred away when unconditional transfer was turned on.
2. Fixed an issue where the power value in the POE field of lldp messages was the actual power value value of the device.
3. Fixed an overflow in the time type variable that caused the device time not to be updated.
4. Fixed the problem of not receiving multicast when unconditional transfer is enabled.
5. Fixed the problem that timed reboot only works once.
6. Fixed the issue that the device could not get voice vlan when both lldp and cdp existed at the same time.
7. Fixed the problem of no certificate for remote phonebook https connection when default certificate is used by provision.
8. Fixed the problem that the soft keys were not displayed when you received a post during a call, exit and then hang up to go back to standby.
9. Fixed the problem that after lcdgui starts up, it receives post before xml get, and the soft key link url can't be used.
10. Fixed the problem of ringing without sound on the get xml broswer page directly after device reboot.
11. Fixed the problem of displaying error when LDAP phonebook failed to call out.
12. Fixed the problem that it takes 2 times to set static IP without plugging in the network cable, and the device changes back to DHCP after reboot.
13. Fixed the issue that when data vlan is turned on and lldp is used, the plugged-in device no longer sends lldp messages and does not switch networks when the lldp message timeout occurs.
14. Fixed the problem that softkey 1, softkey 2, softkey 3, softkey 4, transfer key and up are invalid for setting multicast.
15. Fixed the problem of modifying Spanish translation errors.