

**Paging and Intercom Configuration Guide**

**Directory**

[一、 Introduction 2](#_Toc472)

[二、 Flow Configuration 2](#_Toc26494)

[1、 Configuring FreePBX 2](#_Toc25309)

[① Set Page Groups 2](#_Toc20604)

[三、 Verification of Results 2](#_Toc31324)

1. **Introduction**

In the Paging and Intercom module, you can configure groups of phones that will auto-answer and play the page over their speakers when called from the page group. This module will work with most SIP phones that are supported by the PBX.

1. **Flow Configuration**
2. **Configuring FreePBX**
3. **Set Page Groups**

Create a paging-group number.

**operating steps：**

Applications--》Paging and Intercom--》Add Page Group；




Figure 1 set page groups

1. **Verification of Results**

When users dial 123, extension 1117 and 1122 automatically answer, can hear the broadcast content.